# Software Information
display_name = "Nintendo - SNES / Famicom (higan Accuracy)"
authors = "Near"
supported_extensions = "sfc|smc|gb|gbc|bml|rom"
corename = "nSide (Super Famicom Accuracy)"
license = "GPLv3"
permissions = ""
categories = "Emulator"
display_version = "v105 (Super Famicom Accuracy)"

# Hardware Information
manufacturer = "Nintendo"
systemname = "Super Nintendo Entertainment System"
systemid = "super_nes"

# Libretro Features
supports_no_game = "false"
database = "Nintendo - Super Nintendo Entertainment System|Nintendo - Game Boy|Nintendo - Game Boy Color"
savestate = "true"
savestate_features = "serialized"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "true"
core_options = "true"
core_options_version = "1.0"
load_subsystem = "true"
hw_render = "false"
needs_fullpath = "false"
disk_control = "false"

# Firmware / BIOS
firmware_count = 21
firmware0_desc = "dsp1.data.rom"
firmware0_path = "dsp1.data.rom"
firmware0_opt = "true"
firmware1_desc = "dsp1.program.rom"
firmware1_path = "dsp1.program.rom"
firmware1_opt = "true"
firmware2_desc = "dsp1b.data.rom"
firmware2_path = "dsp1b.data.rom"
firmware2_opt = "true"
firmware3_desc = "dsp1b.program.rom"
firmware3_path = "dsp1b.program.rom"
firmware3_opt = "true"
firmware4_desc = "dsp2.data.rom"
firmware4_path = "dsp2.data.rom"
firmware4_opt = "true"
firmware5_desc = "dsp2.program.rom"
firmware5_path = "dsp2.program.rom"
firmware5_opt = "true"
firmware6_desc = "dsp3.data.rom"
firmware6_path = "dsp3.data.rom"
firmware6_opt = "true"
firmware7_desc = "dsp3.program.rom"
firmware7_path = "dsp3.program.rom"
firmware7_opt = "true"
firmware8_desc = "dsp4.data.rom"
firmware8_path = "dsp4.data.rom"
firmware8_opt = "true"
firmware9_desc = "dsp4.program.rom"
firmware9_path = "dsp4.program.rom"
firmware9_opt = "true"
firmware10_desc = "cx4.data.rom"
firmware10_path = "cx4.data.rom"
firmware10_opt = "true"
firmware11_desc = "st010.data.rom"
firmware11_path = "st010.data.rom"
firmware11_opt = "true"
firmware12_desc = "st010.program.rom"
firmware12_path = "st010.program.rom"
firmware12_opt = "true"
firmware13_desc = "st011.data.rom"
firmware13_path = "st011.data.rom"
firmware13_opt = "true"
firmware14_desc = "st011.program.rom"
firmware14_path = "st011.program.rom"
firmware14_opt = "true"
firmware15_desc = "st018.data.rom"
firmware15_path = "st018.data.rom"
firmware15_opt = "true"
firmware16_desc = "st018.program.rom"
firmware16_path = "st018.program.rom"
firmware16_opt = "true"
firmware17_desc = "SGB1.sfc/sgb1.boot.rom (SGB Boot BIOS)"
firmware17_path = "SGB1.sfc/sgb1.boot.rom"
firmware17_opt = "true"
firmware18_desc = "SGB1.sfc/program.rom (SGB Boot Image)"
firmware18_path = "SGB1.sfc/program.rom"
firmware18_opt = "true"
firmware19_desc = "SGB2.sfc/sgb2.boot.rom (SGB Boot BIOS)"
firmware19_path = "SGB2.sfc/sgb2.boot.rom"
firmware19_opt = "true"
firmware20_desc = "SGB2.sfc/program.rom (SGB Boot Image)"
firmware20_path = "SGB2.sfc/program.rom"
firmware20_opt = "true"
notes = "[1] higan Accuracy uses split ROMS for special chip games.|[*] Notable DSP1/DSP1B Games: Super Mario Kart,  Pilotwings|[*] Notable DSP2 Games: Dungeon Master|[*] Notable DSP3 Games: SD Gundam GX|[*] Notable DSP4 Games: Top Gear 3000|[*] Notable Cx4 Games: Mega Man X2,  Mega Man X3|[2] SGB Emulation needs SGB.sfc/, SGB1.sfc/ or SGB2.sfc/ foltainers in system directory.|SGB1.sfc/ or SGB2.sfc/ can be selected as core options.|GB/GBC ROMs can be loaded directly as ROMs in this core."

description = "higan Accuracy is based on version 105 of the higan emulator suite's SNES/SFC emulator. It includes the demanding dot-based PPU (which is the hallmark of the 'accuracy' profile of this emulator lineage), though the only commercial game that is affected by this is the notorious Air Strike Patrol (A.S.P.). The up-to-date bsnes core is a better choice for most users who are seeking the highest accuracy and it should be quite a bit faster, too."
