filters = 1
filter0 = chorus

# Controls the base delay of the chorus (milliseconds).
# chorus_delay_ms = 25.0
#
# Controls the depth of the delay. The delay will vary between delay_ms +/- depth_ms.
# chorus_depth_ms = 1.0
#
# Frequency of LFO which controls delay.
# chorus_lfo_freq = 0.5
#
# Controls dry/wet-ness of effect. 1.0 = full chorus, 0.0 = no chorus.
# chorus_drywet = 0.8
